{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":10,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[[6,4,6,5],[19,4,19,7],[20,4,20,7],[21,4,21,7],[22,4,22,7],[28,4,28,7],[29,4,29,7],[23,4,23,7],[24,4,24,7],[25,4,25,7],[26,4,26,7],[27,4,27,7]]}
[]
[]
[null,null,null,"COMポートNo.：","COM3"]
[]
[]
[]
[null,null,null,"耐電圧試験器型名："]
[]
[null,null,null,null,null,null,null,"設定電圧範囲"]
[null,null,null,"設定電圧値：",10,"ｋV",null,"0 ～ 10.00kV (7470)"]
[null,null,null,null,null,null,null,"0 ～ 12.00kV (7472)"]
[null,null,null,null,null,null,null,"0 ～ 20.00kV (7473)"]
[null,null,null,"試験時間：",20,"ｓ",null,"0 ～ 20.00kV (7474)"]
[]
[]
[]
[]
[]
[]
[null,null,null,"測定回数","測定データ"]
[null,null,null,1]
[null,null,null,2]
[null,null,null,3]
[null,null,null,4]
[null,null,null,5]
[null,null,null,6]
[null,null,null,7]
[null,null,null,8]
[null,null,null,9]
[null,null,null,10]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}